**764** ABRAMS ET AL.: JOURNAL OF AOAC INTERNATIONAL VOL. 97, NO. 3, 2014

**SPECIAL GUEST EDITOR SECTION**

**Determination of Kjeldahl Nitrogen in Fertilizers by AOAC**

***Official Method*SM 978.02: Effect of Copper Sulfate as a Catalyst**

**DEAN ABRAMS, DAVID METCALF, and MICHAEL H 1**

**OJJATIE**

Tessenderlo Kerley, Inc., Research and Development Department, 2045 N. Forbes Blvd, #106, Tucson, AZ 85745

Downloaded from https://academic.oup.com/jaoac/article/97/3/764/5654772 by guest on 17 May 2022

# In AOAC *Official Method*SM 955.04, Nitrogen (Total) in Fertilizers, Kjeldahl Method, fertilizer materials are analyzed using mercuric oxide or metallic mercury (HgO or Hg) as a catalyst. AOAC *Official Method*SM 970.02, Nitrogen (Total) in Fertilizers is a comprehensive total nitrogen (including nitrate nitrogen) method adding chromium metal. AOAC *Official Method*SM 978.02, Nitrogen (Total) in Fertilizers is a modified comprehensive nitrogen

**method used to measure total nitrogen in fertilizers with two types of catalysts. In this method, either copper sulfate or chromium metal is added to analyze for total Kjeldahl nitrogen. In this study, the part of AOAC *Official Method*SM 978.02 that is for nitrate-free fertilizer products was modified. The objective was to examine the necessity of copper sulfate as a catalyst for the nitrate-free fertilizer products. Copper salts are not environmentally friendly and are considered pollutants. Products such as ammonium sulfate, diammonium phosphate, monoammonium phosphate, urea-containing fertilizers such as isobutylene diurea (IBDU), and urea-triazone fertilizer solutions were examined.**

# The first part of the study was to measure Kjeldahl nitrogen as recommended by AOAC *Official Method*SM 978.02. The second part of the study was to exclude the addition of copper sulfate from AOAC *Official Method*SM 978.02 to examine the necessity of copper sulfate as a catalyst in nitrate-free fertilizers, which was the primary objective. Our findings indicate that copper sulfate can be eliminated

**from the method with no significant difference in the results for the nitrogen content of the fertilizer products.**

he Kjeldahl method was developed in 1883 (1). It is used for the quantitative determination of nitrogen in various chemical substances. It involves the digestion of the nitrogen-containing compounds with sulfuric acid using heat and conversion of the nitrogen to ammonium ions. Potassium sulfate is added to increase the boiling point of the acid solution. The solution is then distilled with caustic soda (NaOH) to liberate ammonia gas, which is absorbed in a sulfuric acid solution. Part of the sulfuric acid solution is neutralized by the

T

Guest edited as a special report from the AOAC Agricultural Community on “Collaborations in New and Improved Methods of Analysis for Plant Food Materials” by Nancy Thiex.

1 Corresponding author’s e-mail: [mhojjatie@tkinet.com](mailto:mhojjatie@tkinet.com) DOI: 10.5740/jaoacint.13-299

evolved ammonia gas, and the excess acid is back-titrated with sodium hydroxide.

There are several AOAC *Official Methods*SM regarding the Kjeldahl digestion (2). AOAC *Official Method*SM **955.04** for total nitrogen in fertilizers includes the use of catalysts such as mercuric oxide or metallic mercury, zinc granules, and zinc dust. Parts C and D of AOAC **955.04** are improved approaches for nitrate-free fertilizer materials and nitrate-containing fertilizer materials, respectively. AOAC *Official Method*SM **970.02** for determination of total nitrogen in fertilizers includes the use of catalysts such as chromium metal and alundum. Alundum is mixture of aluminum oxide, silicate, ferric oxide, potassium oxide, and sodium oxide. AOAC *Official Method*SM **970.03** is applicable to all fertilizers except nitric phosphate compounds and uses Raney nickel powder as a catalyst. AOAC *Official Method*SM **920.03** (magnesium oxide method) and AOAC *Official Method*SM **920.04** (formaldehyde titration method) are used for ammoniacal nitrogen determination in fertilizers.

AOAC *Official Method*SM **978.02** is for the determination of nitrogen (total) in fertilizers (Kjeldahl method) and is a modified comprehensive nitrogen method (Final Action 1984). In this method, there are two ways to measure total nitrogen: one is to add copper sulfate to analyze for total Kjeldahl nitrogen, and the second is to proceed by adding chromium metal to analyze for total nitrogen, including nitrate nitrogen.

The first approach involves the use of anhydrous copper sulfate or copper sulfate pentahydrate catalyst and alundum for the nitrogen determination. Both copper and fused-aluminum oxide are environmentally hazardous materials. The second option is to proceed by adding chromium metal to analyze for total nitrogen, including nitrate nitrogen. Chromium is also an environmentally hazardous substance.

In order to determine whether the use of copper sulfate is necessary, a series of measurements were done with and without copper sulfate catalyst. Early on in an internal series of studies, when determining the total nitrogen in a variety of fertilizers, including ammonium sulfate, monoammonium phosphate (MAP), diammonium phosphate (DAP), urea-containing fertilizers such as isobutylene diurea (IBDU), and urea-containing triazone fertilizers, we determined that the presence of the alundum is not necessary, and it was replaced with glass beads.

# Study Objectives

In this study, several types of fertilizer compounds were selected, and the total Kjeldahl nitrogen for each fertilizer was measured using two procedures to determine the effect of elimination of the copper sulfate catalyst:

1. The procedure outlined in AOAC Method **978.02** (16th

Ed.) is followed in principle (with modifications for scaling

ABRAMS ET AL.: JOURNAL OF AOAC INTERNATIONAL VOL. 97, NO. 3, 2014 **765**

**Table 1. Summarized total Kjeldahl nitrogen measurements by the digestion method**

Cupric sulfate added, 0.4 g

Range of bias

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Compound | Formulation | Yes | No | *n* (x)*a* | Yes | No |
| Ammonium sulfate*b* | 21.18% N | 21.15 ± 0.05 | 21.12 ± 0.08 | 1 (38) | 0.039 | 0.053 |
| TRISERT-K+*c* | 5-0-20-13S | 5.22 ± 0.16 | 5.21 ± 0.17 | 4 (8) | 0.118 | 0.128 |
| TRISERT-KS*c* | 15-0-12-8S | 14.91 ± 0.00 | 14.92 ± 0.01 | 1 (4) | 0.000 | 0.005 |
| N-SURE*c* | 28-0-0 | 28.02 ± 0.15 | 28.03 ± 0.15 | 20 (38) | 0.113 | 0.115 |
| TRISERT-N+*c* | 26-0-0 | 29.93 ± 0.33 | 29.94 ± 0.25 | 1 (4) | 0.235 | 0.180 |
| TRISERT-CB*c* | 26-0-0-5B | 25.86 ± 0.04 | 25.90 ± 0.08 | 1 (4) | 0.025 | 0.055 |
| TRISERT-NB*c* | 26-0-0 | 26.11 ± 0.16 | 26.10 ± 0.19 | 20 (38) | 0.133 | 0.143 |
| FORMOLENE-PLUS*c* | 30-0-0 | 30.00 ± 0.08 | 29.97 ± 0.14 | 8 (10) | 0.058 | 0.120 |
| CR-9*c* | 29.5-0-0 | 29.37 ± 0.00 | 29.34 ± 0.00 | 1 (4) | 0.000 | 0.000 |
| DAP (diammonium phosphate)*d,e* | 18-46-0 | 17.66 ± 0.07 | 17.60 ± 0.07 | 12 (24) | 0.055 | 0.075 |
| MAP (monoammonium phosphate)*d* | 11-52-0 | 10.93 ± 0.18 | 10.97 ± 0.33 | 6 (12) | 0.150 | 0.235 |
| IBDU (1,1ʹ-isobutylene diurea)*f*,*g* | 30-0-0 | 30.47 ± 0.12 | 30.56 ± 0.02 | 2 (8) | 0.085 | 0.012 |

*a* Number of materials with number of replicates in parenthesis. Each material was run in duplicate except the ammonium sulfate.

*b* Aldrich Chemical Co., Milwaukee, WI, Cat. No. 204501, MW = 132.14 g/mole, purity 99.999%.

*c* Tessenderlo Kerley, Inc., Phoenix, AZ.

*d* CF Industries, Plant City, FL.

*e* Mosaic Research and Development, Mosaic Co., Lithia, FL.

*f* Nu-Gro, Grand Rapids, MI.

*g* Wilbur-Ellis Co., Fresno, CA.

down the amounts of samples and reagents used), and the results of analyses are tabulated in Table 1 under a column identified as “Yes” indicating copper sulfate was used.

Downloaded from https://academic.oup.com/jaoac/article/97/3/764/5654772 by guest on 17 May 2022

1. The second procedure also follows the scaled down modification of AOAC **978.02** (16th Ed.), except copper sulfate is deleted from the list of reagents added for digestion. Results of analyses for this procedure are also tabulated in Table 1 under the column identified as “No” indicating no copper sulfate was used.

# Procedure for Determination of Total Kjeldahl Nitrogen in Fertilizers

*(Adopted from AOAC Method 978.02, 16th Ed***.)**

*Step 1—Digestion*

Add 15 g K2SO4 or 12 g anhydrous Na2SO4, 0.4 g anhydrous CuSO4, or 0.6 g CuSO4∙5H2O, and approximately 0.8 g alundum granules. Add 37 mL diluted sulfuric acid with water H2SO4 + H2O (1 + 1, v/v) or 20 mL concentrated sulfuric acid if adequate ventilation is available. Add sufficient test portion mass, precisely 0.1000 to 2.800 g for fertilizers with 30 to 5% nitrogen, respectively. Rinse the inner wall with about 10 mL water. Transfer the flasks to a preheated (400°C) Kjeldahl block digestor and digest the test portions for 75 min.

AOAC *Official Method*SM **955.04** or the subsequent modified versions (**970.02** and **978.02**) does not specify the temperature. It describes using a preheated block in such a way to bring 250 mL water to boiling in 5 min. This corresponds to 400°C.

Modifications of Step 1 included elimination of copper

sulfate and alundum. Because alundum was eliminated, two

glass beads were used to reduce bumping. Also, 7–8 g K2SO4 was used instead of 15 g, and 15 mL concentrated H2SO4 was used instead of 37 mL (1 + 1).

The ratio of K2SO4 and H2SO4 (1 + 1) is approximately

2.5 (37 mL/15 g = 2.466). The amounts were reduced accordingly, but within the same ratio. As a result, 7.5–8 g K2SO4 and 15 mL concentrated H2SO4 were used, and the wall of the digestion tubes was washed with 5–10 mL water, so a total of 20–25 mL H2SO4 (1 + 1) was used instead of 37 mL. This maintains the ratio of K2SO4 to H2SO4 (1 + 1) as prescribed but uses less reagents.

*Step 2—Determination*

Remove the flasks from the heating block and upon cooling (the reaction mixture must be near room temperature) wash the inner wall with 20–30 mL water and mix. Prepare the distillate receiving flask (a 300 mL Erlenmeyer flask) by adding 30 mL of 0.25 N standardized sulfuric acid to trap the expected total nitrogen in the test portion. Add 2–3 drops of methyl purple indicator and install the receiver on the outlet tube of the distillation unit, being sure that the distillate outlet tube end is totally immersed in the standardized acid solution. Install the digestion tube on the distillation unit. Initiate steam generation and slowly dispense about 80 mL (30–35%) sodium hydroxide into the flask. Continue steam distillation until about 250 mL or more of steam condensate has been collected in the receiving flask. This usually requires about 6–8 min. If color changes to green, add more 0.25 N H2SO4 to bring the color back to purple and record the amount of acid added. Titrate to a grey end point

**Table 2. Statistical data for total Kjeldahl nitrogen by the digestion method for different classes of fertilizers**

Cupric sulfate added

Yes No

Group I

Total nitrogen mean

95% confidence

interval for mean SD High Low Median

Absolute deviation

from median Group II

Total nitrogen mean

95% confidence

interval for mean SD High Low Median

Absolute deviation

from median F*a*

**766** ABRAMS ET AL.: JOURNAL OF AOAC INTERNATIONAL VOL. 97, NO. 3, 2014

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| A.S. Group A | 21.1 | 21.1 | 21.2 | 0.051 | 21.3 | 21.1 | 21.1 | 0.037 | A.S. Group B | 21.1 | 21.0 | 21.2 | 0.079 | 21.2 | 20.8 | 21.1 | 0.046 | 0.673 |
| T-K+ Group C | 5.2 | 5.0 | 5.4 | 0.161 | 5.5 | 5.1 | 5.2 | 0.105 | T-K+ Group D | 5.2 | 5.0 | 5.4 | 0.171 | 5.5 | 5.1 | 5.1 | 0.095 | 0.000 |
| T-KS Group E | 14.9 | 14.7 | 15.1 | 0.000 | 14.9 | 14.9 | 14.9 | 0.000 | T-KS Group F | 14.9 | 14.7 | 15.1 | 0.006 | 14.9 | 14.9 | 14.9 | 0.005 | 1.000 |
| N-SURE Group G | 28.0 | 27.9 | 28.1 | 0.153 | 28.2 | 27.6 | 28.1 | 0.110 | N-SURE Group H | 28.0 | 27.9 | 28.1 | 0.149 | 28.3 | 27.8 | 28.0 | 0.115 | –0.006 |
| T-N+ Group I | 29.9 | 29.7 | 30.1 | 0.271 | 30.2 | 29.7 | 29.9 | 0.235 | T-N+ Group J | 29.9 | 29.8 | 30.1 | 0.208 | 30.1 | 29.8 | 29.9 | 0.180 | 0.002 |
| T-CB Group K | 25.9 | 25.7 | 26.1 | 0.029 | 25.9 | 25.8 | 25.9 | 0.025 | T-CB Group L | 25.9 | 25.7 | 26.1 | 0.064 | 25.9 | 25.8 | 25.9 | 0.055 | 0.000 |
| T-NB Group M | 26.1 | 26.0 | 26.2 | 0.165 | 26.5 | 25.9 | 26.1 | 0.127 | T-NB Group N | 26.1 | 26.0 | 26.2 | 0.187 | 26.4 | 25.7 | 26.1 | 0.141 | 0.001 |
| FOR+ Group O | 30.0 | 29.8 | 30.2 | 0.085 | 30.1 | 29.9 | 30.0 | 0.050 | FOR+ Group P | 30.0 | 29.8 | 30.1 | 0.143 | 30.1 | 29.8 | 30.0 | 0.110 | 0.031 |
| CR-9 Group Q | 29.4 | 29.2 | 29.6 | 0.000 | 29.4 | 29.4 | 29.4 | 0.000 | CR-9 Group R | 29.3 | 29.1 | 29.6 | 0.000 | 29.3 | 29.3 | 29.3 | 0.000 | 0.000 |
| DAP Group S | 17.6 | 17.5 | 17.7 | 0.269 | 18.1 | 17.2 | 17.5 | 0.184 | DAP Group T T | 17.5 | 17.4 | 17.7 | 0.284 | 18.1 | 17.3 | 17.5 | 0.200 | 0.013 |
| MAP Group U | 10.9 | 10.8 | 11.1 | 0.178 | 11.1 | 10.7 | 11.0 | 0.132 | MAP Group V | 11.0 | 10.8 | 11.1 | 0.327 | 11.5 | 10.6 | 11.0 | 0.235 | 0.016 |
| IBDU Group W | 30.5 | 30.3 | 30.7 | 0.388 | 30.9 | 30.1 | 30.4 | 0.315 | IBDU Group X | 30.6 | 30.4 | 30.8 | 0.667 | 31.2 | 30.0 | 30.6 | 0.578 | 0.019 |

*a* “F” is determined by pairing each subgroup in Group I with its equivalent subgroup in Group II.

ABRAMS ET AL.: JOURNAL OF AOAC INTERNATIONAL VOL. 97, NO. 3, 2014 **767**

(pH 5.7) with 0.25 N standard NaOH. No modifications were

Downloaded from https://academic.oup.com/jaoac/article/97/3/764/5654772 by guest on 17 May 2022

made to Step 2.

*Step 3—Calculations*

The color of the distillate depends upon the amount of total nitrogen in the test portion, which is a function of the amount of ammonia trapped in the receiver flask. A green color indicates that the acid in the trap was neutralized by the ammonia. At this point, add an additional known amount of standardized H2SO4 to get to the grey end point. The net volume (in mL) of standardized acid would be equal to the total amount of acid initially added to the receiving flask plus the amount of the acid added, after distillation, to reach to the grey end point. A blue or purple color indicates that there is still acid in the receiving flask, and back titration with NaOH is required. The net volume standardized (std) acid would be equal to the amount of acid in the receiving flask minus the amount of base added, after distillation, to reach to the grey end point.

Weight percent total nitrogen is calculated as follows:

Total N, % = (net mL std acid × N of std acid) - (net mL std base × N of std base) × 1.4008

sample weight, g

No modifications were made in Step 3.

# Materials

The nitrogen-containing compounds chosen for these studies are listed in Table 2. These materials represent uniform nitrogen-containing compounds both in liquid and in solid forms. These sets of fertilizers represent both inorganic and organic N-containing fertilizers.

# Results and Discussion

All materials were analyzed using AOAC *Official Method*SM **978.02** as outlined above with and without copper sulfate.

As illustrated in Table 1, there was no significant difference between the results for total Kjeldahl nitrogen with copper sulfate added or without copper sulfate added to the digestion mixture. The low and high analyses numbers, as well as the range of bias, average, and SD, are provided. The average of the analytical results with catalysts and without catalysts is tabulated. For ammonium sulfate, the average is 21.15 ± 0.05% with catalysts and 21.12 ± 0.08% without catalysts. These results and the results for analyses of other products are listed in Table 2.

# Conclusions

For a wide variety of ammonium- and urea-containing fertilizer compounds that contain no nitrate nitrogen sources, the results show that AOAC Method **978.02** can be carried out without the addition of environmentally hazardous catalysts with no significant changes in the analytical data. The resulting data were evaluated using a paired test (3). When the paired test was applied to all the data, no significant differences were observed. The results of the pairing tests are shown in Table 2.

# References

(1) Kjeldahl, J.Z. (1883) *Anal. Chem.* **22**, 366–382

1. *Official Methods of Analysis* (1995) 16th Ed., AOAC INTERNATIONAL, Gaithersburg, MD
2. Keeping, E.S. (1995) *Introduction to Statistical Inference*

(1995) Dover Publications, Inc., Mineola, NY